hilfeMan.html

Configuration software for MP100D / MP12N-S -host communication

Hardware and software requirements for MP100D / MP12N-S -host communication:

- Ethernet (10/100 Mbit) link between host/PC system and MP100D / MP12N-S
- FTP server installed and configured on the host/PC system
- Configuration software on computer of choice (with Java 1.4.0 or higher) in the network

Configuration of MP100D / MP12N-S -host communication:

- Communication Host connection (between MP100D / MP12N-S FTP client and host FTP server)
- File types (assignment of file name extensions and polling cycle times)
  - Request file (command file with read and delete commands)
  - Response file (response file with acknowledgments and error messages)
  - Log file (logs system outputs in addition to contents of response file)
- Data conversion (conversion of inventory management data for read-in/read-out to databases/spreadsheets)
- File transfer (setting defines which file types are converted)