hilfeKom.html

Communication Host connection

- FTP Client:
  1. Active
     The FTP client polls the FTP server installed on the host/PC system for data/request files. FTP data transfer is started.
  2. Inactive
     There is no communication with the FTP server installed on the host/PC system.
     FTP data transfer is stopped.
- TCP/IP addresses:
  There must be a 10/100Mbit Ethernet-LAN connection established between the host/PC system and the MP100D / MP12N-S. Settings on the MP100D / MP12N-S are used to define whether the IP address for the customer's network is obtained via a DHCP server or is permanently set.
  1. MP100D / MP12N-S
     IP in multi-unit network
     Address set manually via MP100D / MP12N-S in the range of 172.16.1.xxx and 172.31.1.xxx
     16 different multi-unit networks can be set this way
     IP in corporate network
     The following can be set via MP100D / MP12N-S:
     - IP address from DHCP server in the corporate network
     - IP address set manually
  2. Host/PC system (FTP server)
     This setting defines the IP address with which the MP100D / MP12N-S addresses the host/PC (FTP server).
     It must be in an accessible network. A default gateway can be set up via MP100D / MP12N-S.
- Login for Host/PC - FTP server:
  The FTP server must have a Login Account for the access data given below
  (assigned in consultation with the system administrator)
  1. User
     The default used here is "MP100D". This can also be changed.
  2. Password
     The default used here is "22488". This can also be changed.
  The MP100D / MP12N-S FTP client logs in to the host/PC FTP server automatically after it has been activated.
- Read/write access rights to FTP server:
  Communication between FTP client and FTP server takes place via 2 file transfer directories.
  The response file (acknowledgment) and the requested files are stored in the inbox.
  The files to be transferred and the request files (inquiries) are stored in the outbox.
  In addition to read/write access rights, the FTP server must also have rights to append files
  1. Inbox path
     The default depends on the operating system and should be adapted to the FTP server settings.
  2. Outbox path
     The default depends on the operating system and should be adapted to the FTP server settings.

Home page