hilfeUeber.html

File transfer Send/Read

Send (Import):
This is where the user defines which file types from the outbox of the host/PC FTP server have to go through the conversion routine when they are sent, and which do not.
Only file types that are formatted in the MP100D / MP12N-S can be selected.
To be able to read in system data from the host/PC system, this must be selected.
An additional password prompt must be answered so that there can be no damage resulting from unauthorized sending of system data. This procedure must be repeated before every send process involving system data.

Read (Export):
This is where the user defines the files that must go through a conversion when they are read out from the MP100D / MP12N-S , before they are stored in the inbox of the FTP server.
Only file types that are formatted in the MP100D / MP12N-S can be selected.

Home page