hilfeRespProt.html

File types Request file

Commands to read/delete data are sent to the MP100D / MP12N-S in this file. The file can be created with a simple ASCII editor.
One command is written per line. More than one command can be sent in each request file.
When the file has been created, it must be copied to the outbox and is read automatically by the MP100D / MP12N-S FTP client and then deleted. The results of a request file are written to the response file and the log file.
Example of a file structure: (e.g. Read single job file xxyy from MP100D / MP12N-S )
READ JOB xxyy filename
The <filename> must not contain a file name extension. This is appended according to the initialization.

Home page